da rulez

* the full assembly and any notes about it should go under the FULL ASSEMBLY folder
* each system gets its own folder. under that folder is the assembled system, its bits, and a folder of rough CAD files, scanned sketches, and notes, which you’ll title ROUGHS if you need to. completed stuff just sits in the system folder
* Naming Convention: Main-ReadMe

(first four letters of the system it’s in**-**a descriptive name of the part)

* read this document periodically bc it is subject to change, and if i ain’t here to tell ya ta look at it ya aint gonna eva look at it. so look at it.

how to keep the folder synced up n shit

* work on one system folder at a time
* keep 2016 Robot CAD Files on your Z drive if you have one (engi kids); the files on your computer MUST mirror the drive files EXACTLY
* make it pretty
* take the old system file, rename it with the date, then place it in OLDBOTS
* place the new system file in ROBOT
* delete the version of a system in OLDBOTS if it’s three or five versions behind

if you only replace/modify one part, you don’t have to go through that whole above

process, but, you have to make sure that you date the part you’re replacing and put it

in its respective place in OLDBOTS